
\documentclass[a4paper]{article}
%\documentclass[a4paper,landscape]{article}

\renewcommand{\familydefault}{\sfdefault}
\usepackage[table]{xcolor}
\definecolor{orange}{rgb}{1, 0.7, 0}
\definecolor{lightgrey}{rgb}{0.925, 0.925, 0.925}

\setlength{\topmargin}{-3cm}
\setlength{\oddsidemargin}{-0.5cm}
\setlength{\evensidemargin}{0cm}
\setlength{\textwidth}{17.5cm}
\setlength{\textheight}{24.5cm}
%\setlength{\textwidth}{25cm}
%\setlength{\textheight}{15cm}
\setlength{\headheight}{84pt}

\usepackage{fancyvrb}
\usepackage{fvextra}
%\usepackage{framed,color}
%\newenvironment{modulelog}{\snugshade\Verbatim}{\endVerbatim\endsnugshade}
\usepackage{adjustbox}
\newenvironment{modulelog}%
{\par\noindent\adjustbox{margin=0ex,bgcolor=shadecolor,margin=0ex}\bgroup\varwidth\linewidth\Verbatim}%
{\endVerbatim\endvarwidth\egroup}
%\usepackage{xcolor}

\renewcommand{\baselinestretch}{1,2}
\setlength{\parindent}{0pt}
\setlength{\parskip}{9pt plus3pt minus3pt}

\usepackage{listings}
\usepackage{color}
\definecolor{bg-partially-covered}{rgb}{1,1,0.6}    % light-yellow
\definecolor{bg-uncovered}{rgb}{1,0.8,0.8}          % light-red
\definecolor{bg-covered}{rgb}{0.95,1,0.95}          % very light-green
\definecolor{bg-clean}{rgb}{1,1,1}                  % white
\definecolor{mygreen}{rgb}{0,0.6,0}
\definecolor{mygray}{rgb}{0.5,0.5,0.5}
\definecolor{mymauve}{rgb}{0.58,0,0.82}
\lstset{ %
  backgroundcolor=\color{white},   % choose the background color; you must add \usepackage{color} or \usepackage{xcolor}; should come as last argument
  basicstyle=\footnotesize,        % the size of the fonts that are used for the code
  breakatwhitespace=false,         % sets if automatic breaks should only happen at whitespace
  breaklines=true,                 % sets automatic line breaking
  captionpos=b,                    % sets the caption-position to bottom
  commentstyle=\color{mygreen},    % comment style
  deletekeywords={...},            % if you want to delete keywords from the given language
  escapeinside={\%*}{*)},          % if you want to add LaTeX within your code
  extendedchars=true,              % lets you use non-ASCII characters; for 8-bits encodings only, does not work with UTF-8
  frame=none,	                   % adds a frame around the code
  keepspaces=true,                 % keeps spaces in text, useful for keeping indentation of code (possibly needs columns=flexible)
  keywordstyle=\color{blue},       % keyword style
  language=Octave,                 % the language of the code
  morekeywords={*,...},            % if you want to add more keywords to the set
  numbers=left,                    % where to put the line-numbers; possible values are (none, left, right)
  numbersep=5pt,                   % how far the line-numbers are from the code
  numberstyle=\tiny\color{mygray}, % the style that is used for the line-numbers
  rulecolor=\color{black},         % if not set, the frame-color may be changed on line-breaks within not-black text (e.g. comments (green here))
  showlines=true,
  showspaces=false,                % show spaces everywhere adding particular underscores; it overrides 'showstringspaces'
  showstringspaces=false,          % underline spaces within strings only
  showtabs=false,                  % show tabs within strings adding particular underscores
  stepnumber=1,                    % the step between two line-numbers. If it's 1, each line will be numbered
  stringstyle=\color{mymauve},     % string literal style
  tabsize=2,	                   % sets default tabsize to 2 spaces
}
\usepackage{hyperref}
\usepackage{longtable}[=v4.13]
\usepackage{tabu}
\usepackage{multicol}
\usepackage{booktabs}
\usepackage{graphicx}
\usepackage{lastpage} % for the number of the last page in the document
\usepackage{fancyhdr}

\fancyhf{}
\renewcommand{\headrulewidth}{0pt}
\renewcommand{\footrulewidth}{0pt}
\lhead{\textcolor{gray}{}}
\chead{\textcolor{gray}{ Unittest for {\tt smart\_brain }}}
\rhead{\textcolor{gray}{}}
\lfoot{\textcolor{gray}{}}
\cfoot{\textcolor{gray}{}}
\rfoot{\textcolor{gray}{\thepage\,/ \pageref{LastPage}}}

\begin{document}

\begin{titlepage}
\date{\today}
\title{
	Unittest for {\tt smart\_brain }
}
\date{\today} 
\maketitle
\thispagestyle{empty}
\newpage
\end{titlepage}

\setcounter{page}{1}
\pagestyle{fancy}

\tableofcontents
\newpage

\section{Test System Information}
\begin{tabu} to \linewidth {lX}
\toprule
{\bf System Information}   & \\
\midrule
Architecture & 64bit \\
Machine & x86\_64 \\
Hostname & ahorn \\
Distribution & Linux Mint 21.1 (vera) \\
System & Linux \\
Kernel & 5.15.0-58-generic (\#64-Ubuntu SMP Thu Jan 5 11:43:13 UTC 2023) \\
Username & dirk \\
Path & /\allowbreak home/\allowbreak dirk/\allowbreak my\_repositories/\allowbreak smarthome/\allowbreak smart\_brain\_test/\allowbreak all.py \\
\bottomrule
\end{tabu}


\section{Summary}
\begin{tabu} to \linewidth {lX}
	\toprule
	Number of tests & {\bf 5}\\
	Number of successfull tests & {\bf 5}\\
	Number of possibly failed tests & \textcolor{black}{\bf 0}\\
	Number of failed tests & \textcolor{black}{\bf 0}\\
	\midrule
	Executionlevel    & unknown\\
	Time consumption  & 4.510s\\
	\bottomrule
\end{tabu}






  \section{\textcolor{green}{Testcases (Success)}}
    
      
        \subsection{ Away mode test: zigbee/\allowbreak gfw/\allowbreak dirk/\allowbreak heating\_valve }
        
          
\paragraph{Testsummary}\mbox{}\\
This test was passed with the state: {\bf \textcolor{green}{Success}}.
\begin{longtabu} to \linewidth {lX}
\toprule
Caller: & /\allowbreak home/\allowbreak dirk/\allowbreak my\_repositories/\allowbreak smarthome/\allowbreak smart\_brain\_test/\allowbreak tests/\allowbreak heating.py (84)\\
Start-Time: & 2023-02-09 07:53:02,566\\
Finished-Time: & 2023-02-09 07:53:03,468\\
Time-Consumption & 0.902s\\
\midrule
\multicolumn{2}{l}{\bf{Testresults:}}\\
\midrule
\bf{\,Info } & Setting preconditions (Default setpoint)\\
\bf{\,\textcolor{green}{Success} } & Away mode is correct (Content False and Type is $<$class 'bool'$>$).\\
\bf{\,Info } & Activating away mode\\
\bf{\,\textcolor{green}{Success} } & Away mode is correct (Content True and Type is $<$class 'bool'$>$).\\
\bf{\,\textcolor{green}{Success} } & Temperature setpoint is correct (Content 20 and Type is $<$class 'int'$>$).\\
\bf{\,Info } & Deactivating away mode\\
\bf{\,\textcolor{green}{Success} } & Away mode is correct (Content False and Type is $<$class 'bool'$>$).\\
\bf{\,\textcolor{green}{Success} } & Temperature setpoint is correct (Content 25 and Type is $<$class 'int'$>$).\\
\bottomrule
\end{longtabu}


\paragraph{Testdetails}\mbox{}\\
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf Info } & Setting preconditions (Default setpoint)\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic videv/gfw/dirk/heating_valve/set_default_temperature and payload true
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/set_default_temperature and payload b'true'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/user_temperature_setpoint and payload b'25'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve/set and payload b'{"current_heating_setpoint": 25}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic zigbee/gfw/dirk/heating_valve and payload {"current_heating_setpoint": 25, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/valve_temperature_setpoint and payload b'25'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve and payload b'{"current_heating_setpoint": 25, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/temperature and payload b'20.7'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Away mode is correct (Content False and Type is $<$class 'bool'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Away mode): False (<class 'bool'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Away mode): result = False (<class 'bool'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf Info } & Activating away mode\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic videv/gfw/dirk/heating_valve/away_mode and payload true
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/away_mode and payload b'true'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve/set and payload b'{"current_heating_setpoint": 20}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic zigbee/gfw/dirk/heating_valve and payload {"current_heating_setpoint": 20, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/valve_temperature_setpoint and payload b'20'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/away_mode and payload b'true'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve and payload b'{"current_heating_setpoint": 20, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/temperature and payload b'20.7'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Away mode is correct (Content True and Type is $<$class 'bool'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Away mode): True (<class 'bool'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Away mode): result = True (<class 'bool'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Temperature setpoint is correct (Content 20 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Temperature setpoint): 20 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Temperature setpoint): result = 20 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf Info } & Deactivating away mode\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic videv/gfw/dirk/heating_valve/away_mode and payload false
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/away_mode and payload b'false'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve/set and payload b'{"current_heating_setpoint": 25}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic zigbee/gfw/dirk/heating_valve and payload {"current_heating_setpoint": 25, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/valve_temperature_setpoint and payload b'25'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/away_mode and payload b'false'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve and payload b'{"current_heating_setpoint": 25, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/temperature and payload b'20.7'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Away mode is correct (Content False and Type is $<$class 'bool'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Away mode): False (<class 'bool'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Away mode): result = False (<class 'bool'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Temperature setpoint is correct (Content 25 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Temperature setpoint): 25 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Temperature setpoint): result = 25 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}

        
      
    
  
    
      
        \subsection{ Boost mode test: zigbee/\allowbreak gfw/\allowbreak dirk/\allowbreak heating\_valve }
        
          
\paragraph{Testsummary}\mbox{}\\
This test was passed with the state: {\bf \textcolor{green}{Success}}.
\begin{longtabu} to \linewidth {lX}
\toprule
Caller: & /\allowbreak home/\allowbreak dirk/\allowbreak my\_repositories/\allowbreak smarthome/\allowbreak smart\_brain\_test/\allowbreak tests/\allowbreak heating.py (107)\\
Start-Time: & 2023-02-09 07:53:03,468\\
Finished-Time: & 2023-02-09 07:53:04,370\\
Time-Consumption & 0.902s\\
\midrule
\multicolumn{2}{l}{\bf{Testresults:}}\\
\midrule
\bf{\,Info } & Setting preconditions (Default setpoint)\\
\bf{\,\textcolor{green}{Success} } & Boost timer is correct (Content 0 and Type is $<$class 'int'$>$).\\
\bf{\,Info } & Activating boost mode\\
\bf{\,\textcolor{green}{Success} } & Boost timer is greater expectation (Content 900 and Type is $<$class 'int'$>$).\\
\bf{\,Info } & Setting postconditions (Default setpoint)\\
\bf{\,\textcolor{green}{Success} } & Boost timer is correct (Content 0 and Type is $<$class 'int'$>$).\\
\bottomrule
\end{longtabu}


\paragraph{Testdetails}\mbox{}\\
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf Info } & Setting preconditions (Default setpoint)\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic videv/gfw/dirk/heating_valve/set_default_temperature and payload true
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/set_default_temperature and payload b'true'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Boost timer is correct (Content 0 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Boost timer): 0 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Boost timer): result = 0 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf Info } & Activating boost mode\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic videv/gfw/dirk/heating_valve/start_boost and payload true
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/start_boost and payload b'true'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/boost_timer and payload b'900'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve/set and payload b'{"current_heating_setpoint": 30}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic zigbee/gfw/dirk/heating_valve and payload {"current_heating_setpoint": 30, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/valve_temperature_setpoint and payload b'30'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve and payload b'{"current_heating_setpoint": 30, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/temperature and payload b'20.7'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Boost timer is greater expectation (Content 900 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Boost timer): 900 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Boost timer): result > 0 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf Info } & Setting postconditions (Default setpoint)\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic videv/gfw/dirk/heating_valve/set_default_temperature and payload true
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/set_default_temperature and payload b'true'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/boost_timer and payload b'0'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve/set and payload b'{"current_heating_setpoint": 25}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic zigbee/gfw/dirk/heating_valve and payload {"current_heating_setpoint": 25, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/valve_temperature_setpoint and payload b'25'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve and payload b'{"current_heating_setpoint": 25, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/temperature and payload b'20.7'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Boost timer is correct (Content 0 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Boost timer): 0 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Boost timer): result = 0 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}

        
      
    
  
    
      
        \subsection{ Default temperature test for device and virtual device: zigbee/\allowbreak gfw/\allowbreak dirk/\allowbreak heating\_valve }
        
          
\paragraph{Testsummary}\mbox{}\\
This test was passed with the state: {\bf \textcolor{green}{Success}}.
\begin{longtabu} to \linewidth {lX}
\toprule
Caller: & /\allowbreak home/\allowbreak dirk/\allowbreak my\_repositories/\allowbreak smarthome/\allowbreak smart\_brain\_test/\allowbreak tests/\allowbreak heating.py (41)\\
Start-Time: & 2023-02-09 07:53:04,370\\
Finished-Time: & 2023-02-09 07:53:04,972\\
Time-Consumption & 0.601s\\
\midrule
\multicolumn{2}{l}{\bf{Testresults:}}\\
\midrule
\bf{\,Info } & Setting preconditions (Valve setpoint to 20.0)\\
\bf{\,\textcolor{green}{Success} } & Valve temperature setpoint (is not default temperature) is correct (Content True and Type is $<$class 'bool'$>$).\\
\bf{\,Info } & Triggering set to default temperature (25.0)\\
\bf{\,\textcolor{green}{Success} } & Valve temperature setpoint is correct (Content 25 and Type is $<$class 'int'$>$).\\
\bottomrule
\end{longtabu}


\paragraph{Testdetails}\mbox{}\\
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf Info } & Setting preconditions (Valve setpoint to 20.0)\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic zigbee/gfw/dirk/heating_valve and payload {"current_heating_setpoint": 20, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve and payload b'{"current_heating_setpoint": 20, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve/set and payload b'{"current_heating_setpoint": 20}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/valve_temperature_setpoint and payload b'20'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/user_temperature_setpoint and payload b'20'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/temperature and payload b'20.7'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Valve temperature setpoint (is not default temperature) is correct (Content True and Type is $<$class 'bool'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Valve temperature setpoint (is not default temperature)): True (<class 'bool'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Valve temperature setpoint (is not default temperature)): result = True (<class 'bool'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf Info } & Triggering set to default temperature (25.0)\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic videv/gfw/dirk/heating_valve/set_default_temperature and payload true
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/set_default_temperature and payload b'true'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/user_temperature_setpoint and payload b'25'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve/set and payload b'{"current_heating_setpoint": 25}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic zigbee/gfw/dirk/heating_valve and payload {"current_heating_setpoint": 25, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/valve_temperature_setpoint and payload b'25'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve and payload b'{"current_heating_setpoint": 25, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/temperature and payload b'20.7'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Valve temperature setpoint is correct (Content 25 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Valve temperature setpoint): 25 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Valve temperature setpoint): result = 25 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}

        
      
    
  
    
      
        \subsection{ Summer mode test: zigbee/\allowbreak gfw/\allowbreak dirk/\allowbreak heating\_valve }
        
          
\paragraph{Testsummary}\mbox{}\\
This test was passed with the state: {\bf \textcolor{green}{Success}}.
\begin{longtabu} to \linewidth {lX}
\toprule
Caller: & /\allowbreak home/\allowbreak dirk/\allowbreak my\_repositories/\allowbreak smarthome/\allowbreak smart\_brain\_test/\allowbreak tests/\allowbreak heating.py (61)\\
Start-Time: & 2023-02-09 07:53:04,972\\
Finished-Time: & 2023-02-09 07:53:05,874\\
Time-Consumption & 0.902s\\
\midrule
\multicolumn{2}{l}{\bf{Testresults:}}\\
\midrule
\bf{\,Info } & Setting preconditions (Default setpoint)\\
\bf{\,\textcolor{green}{Success} } & Summer mode is correct (Content False and Type is $<$class 'bool'$>$).\\
\bf{\,Info } & Activating summer mode\\
\bf{\,\textcolor{green}{Success} } & Summer mode is correct (Content True and Type is $<$class 'bool'$>$).\\
\bf{\,\textcolor{green}{Success} } & Temperature setpoint is correct (Content 5 and Type is $<$class 'int'$>$).\\
\bf{\,Info } & Deactivating summer mode\\
\bf{\,\textcolor{green}{Success} } & Summer mode is correct (Content False and Type is $<$class 'bool'$>$).\\
\bf{\,\textcolor{green}{Success} } & Temperature setpoint is correct (Content 25 and Type is $<$class 'int'$>$).\\
\bottomrule
\end{longtabu}


\paragraph{Testdetails}\mbox{}\\
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf Info } & Setting preconditions (Default setpoint)\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic videv/gfw/dirk/heating_valve/set_default_temperature and payload true
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/set_default_temperature and payload b'true'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Summer mode is correct (Content False and Type is $<$class 'bool'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Summer mode): False (<class 'bool'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Summer mode): result = False (<class 'bool'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf Info } & Activating summer mode\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic videv/gfw/dirk/heating_valve/summer_mode and payload true
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/summer_mode and payload b'true'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve/set and payload b'{"current_heating_setpoint": 5}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic zigbee/gfw/dirk/heating_valve and payload {"current_heating_setpoint": 5, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/valve_temperature_setpoint and payload b'5'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/summer_mode and payload b'true'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve and payload b'{"current_heating_setpoint": 5, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/temperature and payload b'20.7'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Summer mode is correct (Content True and Type is $<$class 'bool'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Summer mode): True (<class 'bool'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Summer mode): result = True (<class 'bool'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Temperature setpoint is correct (Content 5 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Temperature setpoint): 5 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Temperature setpoint): result = 5 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf Info } & Deactivating summer mode\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic videv/gfw/dirk/heating_valve/summer_mode and payload false
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/summer_mode and payload b'false'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve/set and payload b'{"current_heating_setpoint": 25}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic zigbee/gfw/dirk/heating_valve and payload {"current_heating_setpoint": 25, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/valve_temperature_setpoint and payload b'25'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/summer_mode and payload b'false'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve and payload b'{"current_heating_setpoint": 25, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/temperature and payload b'20.7'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Summer mode is correct (Content False and Type is $<$class 'bool'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Summer mode): False (<class 'bool'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Summer mode): result = False (<class 'bool'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Temperature setpoint is correct (Content 25 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Temperature setpoint): 25 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Temperature setpoint): result = 25 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}

        
      
    
  
    
      
        \subsection{ User temperature setpoint test for device and virtual device: zigbee/\allowbreak gfw/\allowbreak dirk/\allowbreak heating\_valve }
        
          
\paragraph{Testsummary}\mbox{}\\
This test was passed with the state: {\bf \textcolor{green}{Success}}.
\begin{longtabu} to \linewidth {lX}
\toprule
Caller: & /\allowbreak home/\allowbreak dirk/\allowbreak my\_repositories/\allowbreak smarthome/\allowbreak smart\_brain\_test/\allowbreak tests/\allowbreak heating.py (17)\\
Start-Time: & 2023-02-09 07:53:05,874\\
Finished-Time: & 2023-02-09 07:53:07,076\\
Time-Consumption & 1.203s\\
\midrule
\multicolumn{2}{l}{\bf{Testresults:}}\\
\midrule
\bf{\,Info } & Changing valve temperature setpoint to '20.0'\\
\bf{\,\textcolor{green}{Success} } & Virtual device valve temperature is correct (Content 20 and Type is $<$class 'int'$>$).\\
\bf{\,\textcolor{green}{Success} } & Virtual device user temperature is correct (Content 20 and Type is $<$class 'int'$>$).\\
\bf{\,Info } & Changing videv user temperature setpoint to '25.0'\\
\bf{\,\textcolor{green}{Success} } & Valve device temperature setpoint is correct (Content 25 and Type is $<$class 'int'$>$).\\
\bf{\,\textcolor{green}{Success} } & Virtual device valve temperature is correct (Content 25 and Type is $<$class 'int'$>$).\\
\bf{\,Info } & Changing valve temperature setpoint to '20.0'\\
\bf{\,\textcolor{green}{Success} } & Virtual device valve temperature is correct (Content 20 and Type is $<$class 'int'$>$).\\
\bf{\,\textcolor{green}{Success} } & Virtual device user temperature is correct (Content 20 and Type is $<$class 'int'$>$).\\
\bf{\,Info } & Changing videv user temperature setpoint to '25.0'\\
\bf{\,\textcolor{green}{Success} } & Valve device temperature setpoint is correct (Content 25 and Type is $<$class 'int'$>$).\\
\bf{\,\textcolor{green}{Success} } & Virtual device valve temperature is correct (Content 25 and Type is $<$class 'int'$>$).\\
\bottomrule
\end{longtabu}


\paragraph{Testdetails}\mbox{}\\
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf Info } & Changing valve temperature setpoint to '20.0'\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic zigbee/gfw/dirk/heating_valve and payload {"current_heating_setpoint": 20, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve and payload b'{"current_heating_setpoint": 20, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve/set and payload b'{"current_heating_setpoint": 20}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/valve_temperature_setpoint and payload b'20'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/user_temperature_setpoint and payload b'20'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/temperature and payload b'20.7'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Virtual device valve temperature is correct (Content 20 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Virtual device valve temperature): 20 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Virtual device valve temperature): result = 20 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Virtual device user temperature is correct (Content 20 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Virtual device user temperature): 20 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Virtual device user temperature): result = 20 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf Info } & Changing videv user temperature setpoint to '25.0'\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic videv/gfw/dirk/heating_valve/user_temperature_setpoint and payload 25
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/user_temperature_setpoint and payload b'25'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve/set and payload b'{"current_heating_setpoint": 25}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic zigbee/gfw/dirk/heating_valve and payload {"current_heating_setpoint": 25, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/valve_temperature_setpoint and payload b'25'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/user_temperature_setpoint and payload b'25'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve and payload b'{"current_heating_setpoint": 25, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/temperature and payload b'20.7'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Valve device temperature setpoint is correct (Content 25 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Valve device temperature setpoint): 25 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Valve device temperature setpoint): result = 25 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Virtual device valve temperature is correct (Content 25 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Virtual device valve temperature): 25 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Virtual device valve temperature): result = 25 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf Info } & Changing valve temperature setpoint to '20.0'\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic zigbee/gfw/dirk/heating_valve and payload {"current_heating_setpoint": 20, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve and payload b'{"current_heating_setpoint": 20, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve/set and payload b'{"current_heating_setpoint": 20}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/valve_temperature_setpoint and payload b'20'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/user_temperature_setpoint and payload b'20'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/temperature and payload b'20.7'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Virtual device valve temperature is correct (Content 20 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Virtual device valve temperature): 20 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Virtual device valve temperature): result = 20 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Virtual device user temperature is correct (Content 20 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Virtual device user temperature): 20 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Virtual device user temperature): result = 20 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf Info } & Changing videv user temperature setpoint to '25.0'\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic videv/gfw/dirk/heating_valve/user_temperature_setpoint and payload 25
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/user_temperature_setpoint and payload b'25'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve/set and payload b'{"current_heating_setpoint": 25}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Sending message with topic zigbee/gfw/dirk/heating_valve and payload {"current_heating_setpoint": 25, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/valve_temperature_setpoint and payload b'25'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/user_temperature_setpoint and payload b'25'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic zigbee/gfw/dirk/heating_valve and payload b'{"current_heating_setpoint": 25, "local_temperature": 20.7, "__type__": "brennenstuhl_heating_valve"}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/temperature and payload b'20.7'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Received message with topic videv/gfw/dirk/heating_valve/__info__ and payload b'{"__type__": "videv_heating", "user_temperature_setpoint": {"control": true, "display": true}, "away_mode": {"control": true, "display": true}, "summer_mode": {"control": true, "display": true}, "start_boost": {"control": true}, "set_default_temperature": {"control": true}, "valve_temperature_setpoint": {"display": true}, "boost_timer": {"display": true}, "temperature": {"display": true}}'
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Valve device temperature setpoint is correct (Content 25 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Valve device temperature setpoint): 25 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Valve device temperature setpoint): result = 25 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}
    \begin{tabu} to \linewidth {lX}
    \toprule
    {\bf \textcolor{green}{Success} } & Virtual device valve temperature is correct (Content 25 and Type is $<$class 'int'$>$).\\
    \bottomrule
    \end{tabu}
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Result (Virtual device valve temperature): 25 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]
        \definecolor{shadecolor}{rgb}{ 0.8 0.8 0.8 }\begin{modulelog}[breaklines=true, breakanywhere=true]
        Expectation (Virtual device valve temperature): result = 25 (<class 'int'>)
        \end{modulelog}
        \vspace*{-0.225cm}\pagebreak[1]

    \vspace*{2.5ex}

        
      
    
  



\end{document}